|  |  |
| --- | --- |
| **Model** | **CKB-02** |
| Comm. Interface | RS-485, RS-232 |
| Protocol | Pelco-D, Pelco-P |
| Address | 0~255 |
| Display | OLED |
| Joystick | 4-axis |
| Power | DC12V |
| Power Consumption | <2W |
| Working Temperature | 0℃ ~ 40℃ |
| Storage Temperature | -20℃ ~ +50℃ |
| Humidity | ≤90% (no condensation) |
| Dimension | 200mm(L) x 120mm(W) x 103mm(H) |
| Net Weight | 0.5kg |
| Baud Rate | 2400bps, 4800bps, 9600bps,19200bps, 38400bps |