|  |  |
| --- | --- |
| **Model** | **NS-TC200U3** |
| Image Sensor | 1/2.8" CMOS, 2.14MP |
| Video Standard | 1920x1080P/60/50/30/25/20/15/10/5  1280x720P/60/50/30/25/20/15/10/5  1024x768P/60/50/30/25/20/15/10/5  800x600P/60/50/30/25/20/15/10/5  640x480P/60/50/30/25/20/15/10/5 |
| Focal | 3.9mm - 46.8mm |
| Iris | F1.6 - F2.8 |
| Optical Zoom | 12X |
| Digital Zoom | 12X |
| Field of View | 72.5°- 6.3° |
| Focus | Auto, Manual, PTZ Trigger AF, One Push |
| Min. Illumination | 0.5Lux |
| Shutter Speed | 1/1 - 1/10,000s |
| Gain | Auto/Manual |
| White Balance | Auto, Indoor, Outdoor, One push, Manual, Automatic tracking, Sodium , Fluorescent |
| AE Control | Auto, Manual, Shutter Priority, Iris Priority, Intelligence |
| BLC | Yes |
| WDR | Yes |
| Noise Reduction | 2D/3D |
| **Pan & Tilt** | |
| Pan Range | -170°~ +170° |
| Tilt Range | -30°~ +90° |
| Pan Speed | 0.1°~120°/s |
| Tilt Speed | 0.1°~80°/s |
| Presets Number | 256 |
| OSD | Yes |
| Image Flip | Yes |
| **Interface** | |
| Video Output | USB3.0, DVI-D |
| Control Interface | USB3.0, RS-232IN/IR, RS-232OUT/RS-485 |
| **General** | |
| Control Protocol | VISCA and Support Daisy Chain, Pelco-D, Pelco-P |
| Address | 0~63 |
| Power Supply | DC12V |
| Dimension | 243mm x 145mm x 163mm |
| Weight | 1.2KG |
| Body Colour | Grey |