|  |  |
| --- | --- |
| **Model** | **NS-NDI20-2K** |
| **Camera** | |
| Image Sensor | 1/2.8" Exmor CMOS, 2.14MP |
| Video Standard (HD) | 1080P60, 1080P30, 1080I60, 720P60  1080P50, 1080P25, 1080I50, 720P50 |
| Focal | f=4.7 mm - 94.0 mm |
| IRIS | F1.6 - F3.5 |
| Optical Zoom | 20X |
| Digital Zoom | 12X |
| Field of View | 59.5°- 2.9° |
| Focus | Auto, Manual, PTZ Trigger AF, One Push |
| Min. Illumination | 0.5lux(Color), 0.1lux(B/W) |
| Shutter Speed | 1/1 ~ 1/10，000s |
| AGC | Auto/Manual |
| White Balance | Auto, Indoor, Outdoor, One Push, Manual, Auto Track |
| AE Control | Auto, Manual, Shutter Priority, Iris Priority, Intelligence |
| **Pan & Tilt** | |
| Pan Range | -170°~ +170° |
| Tilt Range | -30°~ +90° |
| Pan Speed | 0.1°~ 120°/s |
| Tilt Speed | 0.1°~ 80°/s |
| Preset Number | 256 |
| OSD | Yes |
| Image Flip | Yes |
| **Network** | |
| Max. Image Size | 1920 x 1080 |
| Frame Rate | HD: 50Hz: 50fps(1920×1080)  60Hz: 60fps(1920×1080) |
| Video Compression | H.265, H.264 |
| Audio Compression | AAC |
| Protocol | HTTP,  RTSP, RTMP,  RTP,  TCP,  UDP, ONVIF |
| Dual Stream | Support |
| Simultaneous Users | Up to 10 users |
| **Interface** | |
| HD Video Output | HDMI, 3G-SDI |
| Audio | One line in; One line out |
| Ethernet | RJ45(NDI | HX), 100M |
| USB | USB2.0 |
| Locol Storage | TF card, up to 64GB |
| Control Interface | RS-232IN/IR, RS-232OUT/RS-485 |
| **General** | |
| Control Protocol | VISCA and Support Daisy Chain, PELCO-D, PELCO-P |
| Address | 0~63 |
| Power Supply | DC12V |
| Working Temperature | 0°C ~ +40°C |
| Storage Temperature | -20°C ~ +60°C |
| Dimension (W x H x L) | 243mm  x 145mm  x 163mm |
| Weight | 1.2kg |
| Body Colour | Grey |