|  |  |
| --- | --- |
| **Model** | **NS-TC22S-4K30** |
| **4K EPTZ Camera** |
| Image Sensor | 1/2.5"CMOS, 8MP |
| Video Format | YUY2：1920x1080，320x240，640x480，800x600，1024x768，1280x720MJPG：1920x1080，320x240，640x480，800x600，1024 x768，1280x720，3840x2160 |
| Focal | 2.2mm |
| Iris | F2.4 |
| Field of View  | Horizontal 110° |
| Min. Illumination | 1 Lux @ (F1.8, AGC ON)  |
| White Balance | Auto, One Push |
| S / N | ≥50dB |
| AGC | Auto, Manual |
| **Interface** |
| Control Interface | 1 x USB |
| UVC Protocol | UVC1.1 |
| UVC PTZ Control | Support |
| UAC | Support |
| **General** |
| Power Supply | DC 5V |
| Power Consumption | ＜2.5W |
| Work Temp | 0°C ~ + 40°C |
| Storage Temp | -20°C ~ +60°C |
| Dimension（L×W×H） | 208 mm x 56mm x 48mm |
| Weight | 0.22KG |
| Colo | Black |