|  |  |
| --- | --- |
| **Model** | **NS-TC200F** |
| **Tracking Camera** |
| Image Sensor | 1/2.8" Exmor CMOS, 2.14MP |
| Resolution | 1080P60 / 1080P50 / 1080P30 / 1080P25 / 1080I60 / 1080I50 / 720P60 / 720P50 |
| Zoom | Optical: 12X; Digital: 12X |
| Lens | f=3.9mm - 46.8mm; F1.6 - F2.8 |
| Field of View  | Horizontal 72.5°- 6.3° |
| Focus | Auto / Manual / PTZ Trigger AF / One Push |
| Min. Illumination | 0.5lux(Color) |
| Shutter Speed | 1/1 to 1/10,000s |
| AGC | Auto / Manual |
| White Balance | Auto / Indoor / Outdoor / One Push / Manual / Automatic Tracking |
| AE Control | Auto / Manual / Shutter Priority / Iris Priority |
| OSD | English |
| S/N Ratio | ≥50dB |
| **Full View Camera** |
| Image Sensor | 1/2.8" CMOS |
| Effective Pixel | 2.14MP |
| White Balance | Auto |
| Exposure | Auto |
| Field of View | Horizontal: 86°; Vertical: 52° |
| Lens | 2.4mm |
| **Pan & Tilt** |
| Pan Range | -170°~ +170°/s |
| Tilt Range | -30°~ +90°/s |
| Pan Speed | 0.1° ~ 120°/s |
| Tilt Speed | 0.1° ~ 90°/s |
| Presets Number | 256 |
| Control Interface | RS-232 / RS-485 / USB3.0 |
| Ethernet | RJ45, 100M |
| Control Protocol | PELCO-D / VISCA / UVC1.0-1.5 |
| Video Interface | 3G-SDI / DVI-D / USB3.0 |
| **Network** |
| Image Resolution | 1920 \* 1080@60fps |
| Video Compression | H.264 |
| Audio Compression | AAC |
| Protocol | RTMP / RTSP / TCP / UDP / ONVIF / HTTP |
| Local Storage | TF card, max 64GB |
| Dual Stream | Support |
| **General** |
| Power | DC12V,optional POE |
| Working Temperature | 0°C ~ +40°C |
| Storage Temperature | -20°C ~ +60°C |
| Dimension | 243mm x 145mm x 163mm |
| Weight | 1.2KG |
| Body Colour | Grey |